
Install Arduino IDE


V 1.6.6



Just download




Save File to Downloads




Run the executable

When the screen goes black, click on the dialog’s Run button


And get



Select I Agree




Select Next >




Keep the default location, or change

Select Install




Until it is done




Install the Arduino USB Driver

Select Install




And the next

Select Install




Install the libusb-win32

Select Install



And now the Genuino USB Driver

Select Install



And we are done,

Select Close

But wait!

When plugging in the Arduino, a device driver needed to be installed.

So, one must have connection to the internet first time?

